Gas hob installation – Checklist
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Hob Example Quick Checklist
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Comments

‘Appliance Declaration

Have you checked the Gas Appl
Declarations of Compliance Database

nce Supplier

Appliance isolation valve

Does the appliance require an isolation valve?

‘Appliance test point (at
appliance)

Has an appliance test point been installed?

‘Appliance Regulator

Is the appliance regulator set to the correct
operating pressure as per the appliance data
plate.

Hose Assembly (if used as final
connection)

Is the hose of the correct class type, correct
size, and length (1000mm-1200mm), not
passing through wall, floor etc. and does not
have a joint.

Clearances to combustible
material

Do the side and back clearances comply? i.e.
is the burner at least 200mm away from a
combustible surface?

Protection of combustible
materials

Does the installed protection comply? Is there
a compliant splashback installed? Is the
material behind the covering correct.

Toughened Safety Glass used as
a Splashback?

Does the glass comply with AS/NZS 2208 and
is clearly identified as toughened glass?

Rangehood clearance.

Do all clearances comply with AS/NZS 5601
and the manufacturer’s instructions?

Ventilation

s there adequate ventilation? Have
calculations been carried out to verify?

LPG bottle location/installation

I the LPG bottle installation compliant?

LPG injectors

If using LPG, has the appliance been
converted from NG to LPG including changing
jets and altering aeration as required.? Has an
identifying label been attached to the
appliance to identify LPG is being used?

Manufacturer’s instructions

Have all the additional manufacturers
requirements been met?

Gas Type

Is the gas type clearly identified on the
appliance?





